SUPPLY OF EQUIPMENT FOR THE FIT-OUT OF THE COI OFFICES
TECHNICAL SPECIFICATIONS

I. PERFORMANCE BASIS AND EQUIVALENCE FOR ALL LOT
This is a performance-based specification. Any reference to a proprietary product, manufacturer or trademark is indicative of the required level of quality only and is prohibited unless read as followed by the words “or technically equivalent”. Alternative products or standards may be offered only where the tenderer submits a clause-by-clause equivalence statement together with independent test evidence demonstrating equal or superior safety, durability, functionality, interoperability and environmental performance, subject to written approval.
All references to standards mean the latest published edition, including amendments, in force at the tender date. The standards cited (EN, EN ISO, ISO, IEC and applicable Mauritian statutory requirements) establish the required level of quality and shall not restrict competition.
II. CONTRACTOR’S RESPONSIBILITY FOR ALL LOT
The Contractor remains responsible for dimensional verification, coordination, shop drawings, product selection, statutory compliance and delivery of a complete, safe and operational installation. Any item reasonably inferable as necessary for a complete installation is included whether or not individually listed in the price breakdown (décomposition du prix global forfaitaire). 

III. RELATED SERVICE SPECIFICATIONS FOR LOT 2- FURNITURE
1. Scope of works
1.1. Conference/office tables
Design, manufacture, supply and install conference tables complete with tops, frames, modesty components where scheduled, levelling feet, cable management, integrated power/data modules and all accessories.
Dimensions, shape, seating capacity and finish shall follow the approved furniture schedule and room layout. Furniture shall be suitable for repeated institutional office use and future maintenance.
1.2. Conference/office chairs
Supply ergonomic conference/meeting chairs in the scheduled configuration, including frame, seat, back, upholstery, armrests, glides or castors and all adjustments. 
Chairs shall combine professional appearance, comfort, stability and durability for frequent meeting-room use.
1.3. Kitchen loose furniture
Provide kitchen/kitchenette furniture: cabinets and countertops as specified in the specifications, including hardware, brackets, technical cutouts as needed, waterproofing, coordination, and installation.
The supply must prioritize hygiene, moisture resistance, safe access, ease of cleaning, durable commercial-grade hardware, and efficient use of space.
2. Applicable standards
2.1. Conference/office tables
Comply with the latest editions and amendments of the standards listed below and other standards demonstrably necessary for a complete compliant system.
· EN 527-1 and EN 527-2 – Office work tables: dimensions, safety, strength and durability.
· EN 15372 – Strength, durability and safety of non-domestic tables.
· EN 1730 – Test methods for tables.
· EN 438 series – High-pressure decorative laminates, where used.
· EN 717-1 or current equivalent – Formaldehyde emissions from wood-based panels.
· EN IEC 62368-1 – Safety of integrated audiovisual/ICT power modules where applicable

2.2. Conference/office chairs
Comply with the latest editions and amendments of the standards listed below and other standards demonstrably necessary for a complete compliant system.
· EN 16139 – Strength, durability and safety requirements for non-domestic seating.
· EN 1728 – Test methods for strength and durability of seating.
· EN 1022 – Determination of stability.
· EN 1335-1 and EN 1335-2 – Office work chairs where adjustable task-type conference chairs are specified.
· EN 1021-1 and EN 1021-2 – Ignitability of upholstered furniture by cigarette and match-flame equivalents.
· EN ISO 12947 series – Martindale abrasion resistance of upholstery fabrics.

2.3. Kitchen loose furniture
Comply with the latest editions and amendments of the standards listed below and other standards demonstrably necessary for a complete compliant system.
· EN 14749 – Safety requirements and test methods for domestic and kitchen storage units and worktops.
· EN 16121 and EN 16122 – Safety, strength, durability and stability of non-domestic storage furniture.
· EN 1116 – Coordinating sizes for kitchen furniture and appliances.
· EN 438 series – High-pressure decorative laminates.
· EN 312 – Particleboards; EN 622 series – Fibreboards, where applicable.
· EN 13310 – Kitchen sinks: functional requirements and test methods.
· EN 12521 or EN 15372 and EN 16139 – Loose tables and seating, as applicable

3. Execution and installation
3.1. Conference/office tables
The dimensions of the tables and the clear spaces around the seats must be compatible.
On-site assembly must allow for subsequent disassembly without causing damage.
On-site installation includes leveling the tables, aligning them, and securing the cable covers to prevent any tripping hazards.
Protect surfaces until the premises are handed back and clean them using approved cleaning products.

3.2.  Conference/office chairs
Submit a full production sample for ergonomic and finish approval before order.
Deliver fully assembled or assemble using manufacturer-approved fasteners and torque settings.
Adjust moving parts, verify castor suitability and remove packaging without scratching floors.
Provide felt or polymer glides for fixed chairs on hard floors and retain spare glides/castors.

4. Inspection and testing
4.1. Conference/office tables
Review manufacturer test evidence or independent test certificate to relevant EN requirements.
Inspect dimensions, stability, finish, joints, cable access and power/data operation.
Apply a practical distributed load and edge load demonstration where requested without permanent deformation or instability.
4.2. Conference/office chairs
Review product test reports and declared maximum user mass.
Inspect each chair for stability, finish, stitching and correct operation.
Randomly function-test at least 10% of chairs, minimum three units, including swivel, tilt and height adjustment where applicable.
4.3. Kitchen loose furniture
Approve one representative cabinet/finish sample and hardware set.
Inspect carcass materials, edge sealing, fixings and worktop joints before final acceptance.
Load-test selected shelves where requested.
5. Acceptance criteria
5.1. Conference/office tables
Correct approved size, capacity, colour and finish; top flat and joints tight.
No rocking, sharp edges, exposed fasteners, chips, glue residue, colour mismatch or visible cable disorder.
All lids, modules and access panels operate smoothly; table remains stable with equipment and users in normal positions.
Care instructions, warranty and spare keys/tools supplied.
5.2. Conference/office chairs
Approved model and finish, consistent colour and dimensions.
No rocking, sharp edges, loose fasteners, upholstery damage, visible moulding defects or abnormal noise.
All controls operate smoothly and chair returns to stable position.
Minimum 2% spare glides/castors and care instructions supplied.
5.3. Kitchen loose furniture
Cabinets level, plumb and aligned with consistent reveals; doors/drawers operate without binding.
No chipped edges, swelling, scratches, open joints, unsupported spans, exposed raw board or sealant smears.
Worktops and upstands continuous, hygienic and fully sealed; sinks stable and watertight.
Loose furniture stable, undamaged and consistent with approved samples
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